Please read these instructions about LaCie Network Assistant 1.1 for linux.



The software was tested on ubuntu 8.04, mandriva, and Suze, 32bits version.




--Installation--



To install LaCie Network Assistant, just double click on the .package file. You might need to check the file has execution permissions.If not, right click on the file, choose "properties", in the "permissions" settings check "allow executing file as program". 
Upon opening the .package, if the autopackage tools are not installed in your system, the installer will automatically offer you to install it.





--Configuration--



1/ If you have a 64bits system, you will need the Avahi libraries for 32bits.



2/ Mandriva and suze automatically close ports for Avahi. The application can be launched but it does not list devices on your network. In this case you should open the right port for avahi (UDP 5353). We do not advise you to deactivate your firewall.



3/ If you cannot mount volumes, make sure you have "smbfs" installed.




www.lacie.com







