SeaChest_Firmware.Win.txt                                 Revision: 18-Oct-2018
===============================================================================
 SeaChest_Firmware for Windows - Seagate drive utilities
 Copyright (c) 2014-2018 Seagate Technology LLC and/or its Affiliates, All Rights Reserved
 SeaChest_Firmware Version: 2.5.4
 Build Date: Oct 18 2018
===============================================================================
Welcome to Seagate's SeaChest_Firmware diagnostic software.

SeaChest_Firmware is a comprehensive command line tool that can be used to
update firmware, also known as microcode, on Seagate disk drives (this includes
Seagate, Maxtor, Samsung and LaCie).

Seagate products are run by firmware.  Having the latest firmware can improve
performance and or reliability of your product.  Seagate recommends applying
new firmware to enhance the performance and or reliability of your drive.  Like
any software, firmware is improved over time and problems are also fixed. 
Every drive family has a couple of firmware releases during the life of the
product.  Please check in regularly to determine if new firmware is available
for your drive.

SeaChest_Firmware allows for both single drive and sequential batch mode
firmware download.

NOTE: Windows severely restricts downloading firmware to SATA drives.  Please
see the section below "Windows Restrictions Over SATA Firmware Downloads".
SeaChest_Firmware may not be fully functional on non-Seagate drives.

This User Guide file contains important information about SeaChest_Firmware.
Please read this entire file before using this software.

If this is your drive, you should always keep a current backup of your
important data.

Be very careful using SeaChest_Firmware. Power failure during a firmware
download will cause data loss. Never apply firmware to a drive unless you are
certain that the firmware data file is specifically prepared for your drive.
Seagate is not responsible for lost user data.

Usage
=====
        SeaChest_Firmware [-d <device>] {arguments} {options}

Examples
========
        SeaChest_Firmware --scan
        SeaChest_Firmware -d PD2 -i
        SeaChest_Firmware -d PD2 --fwdlInfo
        SeaChest_Firmware -d PD2 --downloadFW fwfilename
        SeaChest_Firmware -d PD2 --fwdlConfig configfile.cfs


Utility arguments
=================
        -s, --scan
                Scan the system and list all storage devices with Physical
                Device assignments. Shows model, serial and firmware numbers.
                If your device is not listed on a scan immediately after
                booting, then wait 10 seconds and run it again.

        -S, --Scan   (note the capital letter S)
                This option is the same as --scan or -s, however it will also
                perform a low level rescan to pick up other devices. This
                low-level rescan may wake devices from low power states and may
                cause the OS to re-enumerate them. Use this diagnostic option
                when a device is plugged in and not discovered in a normal scan.

                NOTE: A low-level rescan may not be available on all interfaces
                or all OSs.  The low-level rescan is not guaranteed to find
                additional devices in the system when the device is unable to
                come to a ready state.

        -F, --scanFlags [option list]
                Use this option with -s to control the output from scan with the
                options listed below. Multiple options can be combined.
                     ata            - show only ATA (SATA) devices
                     usb            - show only USB devices
                     scsi           - show only SCSI (SAS)) devices
                     interfaceATA   - show devices on an ATA interface
                     interfaceUSB   - show devices on a USB interface
                     interfaceSCSI  - show devices on a SCSI or SAS interface
                     ignoreCSMI     - do not scan for any CSMI devices
                     allowDuplicates - allow drives with both CSMI and PD
                                       handles to show up multiple times in the
                                       list.

                Examples of combining two options:
                     -s --scanFlags usb scsi  - show only USB and SAS devices
                     --scan -F ata interfaceSCSI  - show only SATA nearline
                        drives on a SAS adapter

        -d, --device <device handle>
                Use this option with all commands, except --scan, to specify
                the PD physical device handle (target drive) on which to
                perform an operation. See the section below 'Tool Usage Hints'
                for information about defining multiple device handles.

                Example: -d PD0, or -d PD3

        -i, --deviceInfo
                Show information and features for the storage device. USB
                devices will show the product name, serial and firmware numbers
                as communicated by the USB-SATA bridge.  Add --usbChildInfo
                to display details about the drive within the USB enclosure.

        --SATInfo                       (SATA only)
                Displays SATA device information on any interface using both
                SCSI Inquiry/VPD/Log reported data (translated according to
                SAT) and the ATA Identify/Log reported data.

        --testUnitReady
                A simple check to see if the device responds to commands from
                interface.  Ready or Not Ready are the outputs.  Not Ready
                results will also include the full SCSI Sense Code.

        --fwdlInfo
                Use this option to show the firmware download support
                information for a drive.

        --downloadFW [firmware filename]    (Seagate Only)
                Download firmware to a Seagate storage product. Use only
                Seagate authorized firmware data files which are designated for
                the specific model drive. Improper use of this option may harm
                a device and or its data. You may specify the path if the
                firmware data file is in a different location. This option will
                use segmented download by default. Use the --downloadMode
                option to specify a different download mode.

                Please see the section below "Windows Restrictions Over SATA
                Firmware Downloads".

        --downloadMode [full | segmented | deferred]    (Seagate Only)
                Use this command along with the --downloadFW option to set the
                firmware download mode.

                Supported Modes:
                     full      - Performs a download in one large transfer to
                                 the device.
                     segmented - Downloads the firmware in multiple segments to
                                 the device. (Most compatible)
                     deferred  - Performs a segmented download to the device,
                                 but does not activate the new firmware until a
                                 power cycle or activate command is sent. Drives
                                 with this feature are not common. See
                                 --activateFW.

                Note: See the --modelMatch and --onlyFW utility options which
                may assist in creating commands to update multiple similar
                drives.

        --activateFW     (Seagate Only)
                Use this option to issue the command to activate code that was
                sent to the drive using a deferred download command. This will
                immediately activate the new code on the drive. You can use
                this along with a --downloadFW and --downloadMode deferred to
                automatically issue the activate command after the deferred
                download has completed.

        --fwdlConfig [config file]      (Seagate Only)
                Use this option to specify a configuration file to perform an
                update based on a firmware match on multiple drives or a single
                drive in the system.  You may specify the path if the file is
                in a different location. Configuration files consist of model
                numbers, previous compatible firmware and the appropriate
                matching new firmware.  Configuration files may be written to
                support multiple models at a time.  See the section below
                "Firmware Configuration Files" for more information on this
                subject.

        --fwdlDryRun
                Use this option to compare a given config file to the drives in
                a system without performing a firmware update. This can be used
                to check if any drives in the system require an update.

        --fwdlSegSize [segment size in 512B blocks]     (Seagate Only)
                Use this option to specify a segment size in 512B blocks to use
                for a segmented or deferred download. This option will not
                affect an immediate download (full buffer at once). The default
                segment size used is 64. Larger segment sizes may be faster,
                however they may also be incompatible with controllers or
                drivers in the system. Smaller values are more likely to be
                compatible, but also slower. Use this option if the default
                used by the tool is not working correctly for firmware updates.

        --firmwareSlot/--fwBufferID slot#               (Seagate Only)
                Use this option to specify a firmware slot (NVMe) or a buffer
                ID (SCSI) along with the --downloadMode (SCSI) or --activateFW
                (NVMe & SCSI) options.  If this option is not used, a value of
                zero will be used instead, which means the drive will
                automatically select the slot number.

        --calculateFileHash [file]
                Use this option to calculate the hash of a file. The following
                hashes are computed and shown on the screen:
                    MD5
                    SHA1
                    SHA2_224
                    SHA2_256
                    SHA2_384
                    SHA2_512

        --allowFlexibleFWDLAPIUse
                This option is used to control when to use the Windows 10+
                Firmware Download API calls. Default behavior is to only use
                this call when the interface and drive and command all match.
                The default behavior means that only ATA drives on an ATA
                interface with a ATA download command will use this call. SCSI
                SAS drives with a supported write buffer command will also use
                this call. Using this option allows a detected ATA drive on any
                interface to use this call if the OS/driver supports it
                regardless of the command being sent by the opensea-transport
                library.

Utility Options
===============
        -h, --help
                Show utility options and example usage (this output you see now)

        -v [0-4], --verbose [0 | 1 | 2 | 3 | 4]
                Show verbose information. Verbosity levels are
                0 - quiet,
                1 - default
                2 - command descriptions
                3 - command descriptions and values
                4 - command descriptions, values, and data buffers.

                Example: -v 3 or --verbose 3

        -q, --quiet
                Run SeaChest in quiet mode. This is the same as -v0
                or --verbose 0

        -V, --version
                Show SeaChest version and copyright information & exit

        --license
                Display the Seagate End User License Agreement (EULA).

        --echoCommandLine
                Shows the command line above the banner in the standard output.
                Useful when saving output to logs.

        --enableLegacyUSBPassthrough
                Only use this option on old USB or IEEE1394 (Firewire) products
                that do not otherwise work with the tool. This option will
                enable a trial and error method that attempts sending various
                ATA Identify commands through vendor specific means. Because of
                this, certain products may respond in unintended ways since
                they may interpret these commands differently than the bridge
                chip the command was designed for.

        --sat12byte
                This forces the lower layer code to issue SAT spec ATA
                Pass-through 12-byte commands when possible instead of 16-byte
                commands.  By default, 16-byte commands are always used for ATA
                Pass-through.  USB products may need this option as a
                workaround if the default does not perform.

        --onlySeagate
                Use this option to match only Seagate drives for the options
                provided. May also be used with the --scan command.

        --modelMatch [model Number]
                Use this option to run on all drives matching the provided
                model number. This option will provide a closest match although
                an exact match is preferred. Ex: ST500 will match ST500LM0001.
                The option --childModelMatch may be used to match drives in USB
                enclosures.

                Note: See the section below 'Tool Usage Hints' for information
                about defining multiple device handles.

        --onlyFW [firmware revision]
                Use this option to run on all drives matching the provided
                firmware revision. This option will only do an exact match.
                The option --childOnlyFW may be used to match drives in USB
                enclosures.

        --newFW [firmware revision]
                Use this option to skip drives matching the provided firmware
                revision. This option will only do an exact match. This option
                should be used to skip performing an update if a drive already
                has this firmware revision loaded. The option --childNewFW may
                be used to match drives in USB enclosures.

        --forceATA
                Using this option will force the current drive to be treated as
                a ATA drive. Only ATA commands will be used to talk to the
                drive.

        --forceATADMA   (SATA Only)
                Using this option will force the tool to issue SAT commands to
                ATA device using the protocol set to DMA whenever possible (on
                DMA commands). This option can be combined with --forceATA.

        --forceATAPIO   (SATA Only)
                Using this option will force the tool to issue PIO commands to
                ATA device when possible. This option can be combined with
                --forceATA.

        --forceATAUDMA  (SATA Only)
                Using this option will force the tool to issue SAT commands to
                ATA device using the protocol set to UDMA whenever possible (on
                DMA commands). This option can be combined with --forceATA.

        --forceSCSI
                Using this option will force the current drive to be treated as
                a SCSI drive. Only SCSI commands will be used to talk to the
                drive.

        --csmiIgnorePort
                Use this option to force setting the "ignore Port" flag for the
                port identifier in a CSMI passthrough command. This option can
                be combined with --csmiUsePort which will force the passthrough
                to rely on only the SAS address. This flag is intended to help
                troubleshoot or improve CSMI compatibility on systems that are
                otherwise not functional.

        --csmiUsePort
                Use this option to force setting the "Use Port" flag for the
                PHY identifier in a CSMI passthrough command. This option can
                be combined with --csmiIgnorePort which will force the
                passthrough to rely on only the SAS address. This flag is
                intended to help troubleshoot or improve CSMI compatibility on
                systems that are otherwise not functional.

        --csmiVerbose
                Use this option to show some verbose output when running the
                tool on a CSMI handle. The debugging information shown will be
                specific to the CSMI passthrough mechanism and may be useful
                when troubleshooting system/driver compatibility issues.

Return codes
============
        0       No Error Found
        1       Error in command line options
        2       Invalid Device Handle or Missing Device Handle
        3       Operation Failure
        4       Operation not supported
        5       Operation Aborted
        6       File Path Not Found
        7       Cannot Open File
        8       File Already Exists
        ---SeaChest_Firmware specific exit codes---
        32 = Firmware Download Complete
        33 = Deferred Firmware Download Complete
        34 = Deferred Code Activated
        35 = No Drive or Firmware match found
        36 = Model number matched, but Firmware mismatched
        37 = Firmware File Hash Error
        38 = Firmware Already up to date
        39 = Firmware Match Found for update
        40 = Firmware Match Found for update - deferred update supported
        Anything else = unknown error

================
Tool Usage Hints
================
See Sample Output examples below.

First, run the SeaChest -s option to determine what physical device assignment
lines up to your disk drive. This option will also show you other details about
the drive including the current firmware revision. Like this:

Vendor     Handle   Model Number        Serial Number     FwRev
IDE        PD0      ST94813AS           3AA043KP          3.03
SEAGATE    PD1      ST1000NM0011        ZAA15VAS          SN03

You can use SeaChest -s --onlySeagate to limit the display to just Seagate.

All utility arguments will require you to identify the specific drive by
providing the physical device handle (-d, --device).

For example, SeaChest -d PD2 --shortDST --poll

You may combine multiple tests with a single command line.  For example,
SeaChest_SMART -d PD0 -i --smartCheck runs both identify and SMART.

Multiple device handles can be given by adding -d PD# for each additional
handle.  Devices are processed in sequential order.  For example,
SeaChest_Basics -d PD0 -d PD3 -i runs identify on these two devices.

Caution: All device handles may be specified.  However, great care should be
taken to fully anticipate the consequences of running a command on all storage
devices in a system.  For example, a command to erase data on all drives could
be catastrophic or exactly what you want. The shortcut to select all devices is
-d all.  Seagate is not responsible for lost user data.  Along with the
designation for all devices, you can narrow the tasks to specific types of
drives by using the --onlySeagate, --modelMatch and --onlyFW filters.

All Windows version tools support finding CSMI devices and talking to them like
you would a normal device.  The scan output will show all drives it detects
ONCE. CSMI device handles have a structure like SCSI0:1.  If a drive has both a
PD? and SCSI?:? handle, then SeaChest will show the PD handle instead of the
SCSI (CSMI) handle.

When drives are in a RAID, the PD device handle is usually not available and
the CSMI handle may provide an alternate way to talk to the drive.  Just
because a device has a CSMI handle doesn't mean it is part of a RAID.

If you want to see both handles, add --scanFlags allowDuplicates to the command
line.  If you don't want to see any CSMI devices, add --scanFlags ignoreCSMI to
the command line.  SeaChest_Info -d SCSI?:? --csmiInfo is useful when
troubleshooting CSMI device handles questions.

Tests which alter the firmware or erase user data on the drive are limited to
Seagate-only products which include Seagate, Maxtor, Samsung and LaCie.

Tests which take a very long time to complete or erase all user data on the
drive will require a longer command line argument than indicated in the --help
output to the screen.  This approach is taken to eliminate the possibility of
accidental data loss or the commitment of long test times. The longer command
arguments are similar to "I-understand-this-command-will-take-a-long-time" or
"I-understand-this-command-will-erase-all-data".

Advanced SAS installations may use dual ports.  These are listed as Port 0 and
Port 1 on the device information report. When both ports are active, each one
may have a unique /dev/sg designation.  The scan option may indicate that there
are two drives in the system with the same serial number.  Dual port
installations will also report two different Worldwide Numbers (WWN).

Windows Restrictions Over SATA Firmware Downloads
-------------------------------------------------
You should not attempt downloading firmware to a SATA disk drive in the Windows
operating system unless the drive supports the 'deferred' mode.  You define the
mode with the SeaChest command line option '--downloadMode deferred'.  If the
drive does not support deferred mode then the command will be aborted.  Windows
may not be so restrictive on secondary, non-boot SATA drives or SATA drives
attached to host bus adapters (HBAs, controllers, USB, etc).

If you force a primary SATA boot drive to download firmware in Windows using a
different --downloadMode setting, then the result will likely be a BSOD (blue
screen of death) system crash.  This is because the legacy SATA firmware
download modes require the drive to spin down and then back up and the
momentary disappearance of the drive causes the operating system to crash.
Windows is actually protecting the system when it thinks the drive has stopped
responding (see wikis about Ring 0 Protection).

The 'deferred' mode does not spin down the drive.  Instead, the drive waits for
a future reboot of the system and self-activates the firmware at that time.
Other operating systems may utilize the SeaChest --activateFW command to
trigger the switch to the new firmware version.

============================
Firmware Configuration Files
============================
There are two types of SeaChest_Firmware configuration (config) files:
encrypted CFS and plain text CFG.

Seagate-prepared configuration files are encrypted and carry the file extension
CFS.  Seagate does not decrypt or disclose the contents of its CFS files.

Alternatively, you may prepare your own plain text configuration files which
must use the file extension CFG.  SeaChest_Firmware configuration files are
simple text with multiple lines. Each line defines a model and previous
firmware match up to a new firmware data file.  The structure of each line is
this:

  fullModelNumber;$FWREV$oldFwVersion;fwDataFile;(optional)$FWREV$newFwVersion

No spaces, the first $FWREV$ and all three semi-colons (;) are mandatory.

Note: The full model number is the ELECTRONIC version.  The label shows a
shorter version which may not include all of the necessary digits.  When you
run SeaChest -s or --scan the output will display the full electronic model
number.  For example the label may show ST4000DX001 but the full model is
actually ST4000DX001-1CE168.  You must use the full model numbers as given by
the --scan command.

The --scan commmand also shows the current firmware, such as CC46 or SN03 or
0002 or 0001SDM7.  There are several possible variations.  This corresponds to
the old firmware version.  You must precede the old firmware version with these
exact characters $FWREV$, like $FWREV$0001SDM7.

Seagate is the only authorized source for a firmware data file. The file name
and or other documentation should provide the new firmware version for the file.

The last section of the data line is optional, the new firmware version.  If
you include this information correctly, then SeaChest_Firmware may give a
message stating that the drive already has the new firmware.  If you omit the
new firmware details then you must still end the text string with a semi-colon
(;).

For example, this is a four-line configuration file for three different models
and three different firmware data files (not all model numbers have the longer
electronic version):

ST4000DX001-1CE168;$FWREV$CC42;BarracudaXT-CC44.LOD;$FWREV$CC44
ST4000DX001-1CE168;$FWREV$CC43;BarracudaXT-CC44.LOD;$FWREV$CC44
ST120FP0021;$FWREV$B770;SSD-B775.BIN;
ST4000NM0043;$FWREV$0004;Constellation3TB-0005.lod;$FWREV$0005

Remember, no spaces, the first $FWREV$ and all three semi-colons (;) are
mandatory.

Caution:  Firmware download configuration files assume you have knowledge about
which models are compatible with the associated firmware files.  If you are
unsure about the compatibility then you should NOT attempt to download the
firmware to the drive.  Never apply firmware to a drive unless you are certain
that the firmware data file is specifically prepared for your drive. Be very
careful using SeaChest_Firmware. Power failure during a firmware download will
cause data loss. Seagate is not responsible for lost user data.

Finally, you may optionally add a hash check calculation on the firmware data
file to the SeaChest_Firmware configuration file.  Simply, run the
--calculateFileHash option on the firmware data file.  For example, run a MD5
calculation on the file and then add "@MD5=61b33014f2d2a4f9553f6ef64fb82e31"
(substituting your calculation) immediately following the file name, before the
semi-colon (;).  For example:

ST4000DX001-1CE168;$FWREV$CC43;BarracudaXT-CC44.LOD@MD5=61b33014f2d2a4f9553f6ef64fb82e31;$FWREV$CC44

SeaChest_Firmware will compare its own MD5 calculation to the value in the
configuration file and if they do not match then the procedure will abort.  Six
types of hash calculations are supported up to SHA2_512.

===================
General Usage Hints
===================
The tool will require Administrative privileges to run.
Also, verify that the tool has executable rights.

Remember that the command line arguments are cAsE SeNsiTiVe.

Save a log file by redirecting the screen output to a text file by adding space
&>test.log at the end of your command line. Choose your own file name. To
append the screen output to an existing log file use >>test.log.

To save a log and display results at the conclusion of the tests, you can use
the powershell "tee" command. Tee command writes to the STDOUT and to a file.

For example:
powershell ".\SeaChest --echoCommandLine -d PD1 --smartCheck | tee -append mySeaChestLog.txt"

Setup for Windows
-----------------
The SeaChest Utilities Setup places all of the files at "C:\Program
Files\Seagate\SeaChest" and adds an icon on the Desktop.  Clicking the icon
will open a Windows command prompt in Administrator mode at this location.
From there you will need to type the full command line for the tool and device
and options to run the test you require.  See the various SeaChest Help
documentation for descriptions and examples of the various commands.

Manual Launch for Windows
-------------------------
An individual SeaChest utility for Windows cannot be launched by just clicking
on the file name. If started that way, the SeaChest utility will briefly show a
black window box and quickly close.  That is what happens when trying to run it
from the Windows File Manager.

This is a command line tool and the requirement is to open a Command Prompt as
Administrator.  There are two easy ways to do this:
  1. Windows Accessories, right-click the Command Prompt icon and select Run as
     Administrator.
  2. Click Windows Start. In the Start Search box, type cmd, and then press
     CTRL+SHIFT+ENTER.

Then change drives or directory to where the SeaChest utility is located and
run the tool file name from there.

=============
Sample Output
=============

SATA HDD Device Information:

SeaChest_Firmware -i -d PD1
===============================================================================
 SeaChest - Seagate drive utilities
 Copyright (c) 2014-2018 Seagate Technology LLC and/or its Affiliates, All Rights Reserved
===============================================================================
        Model Number: ST4000DX001-1CE168
        Serial Number: ZQ3034X7R
        Firmware Revision: CC44
        World Wide Name: 500Q0C5007A5FCF19
        Drive Capacity (TB/TiB): 4.00/3.64
        Native Drive Capacity (TB/TiB): 4.00/3.64
        Temperature Data:
                Current Temperature (C): 25
                Highest Temperature (C): 40
                Lowest Temperature (C): 18
        Humidity Data:
                Current Humidity (%): Not Reported
                Highest Humidity (%): Not Reported
                Lowest Humidity (%): Not Reported
        Power On Time:  4 days 1 hour
        Power On Hours: 97.00
        MaxLBA: 7814037167
        Native MaxLBA: 7814037167
        Logical Sector Size (B): 512
        Physical Sector Size (B): 4096
        Sector Alignment: 0
        Rotation Rate (RPM): 5900
        Form Factor (inch): 3.5
        Last DST information:
                Time since last DST (hours): 0.00
                DST Status/Result: 0x0
                DST Test run: 0x1
        Interface speed:
                Max Speed (Gb/s): 6.0
                Negotiated Speed (Gb/s): 6.0
        Annualized Workload Rate (TB/yr): 2.51
        Total Bytes Read (GB): 6.65
        Total Bytes Written (GB): 21.27
        Drive Reported Utilization (%): Not Reported
        Encryption Support: Not Supported
        Cache Size (MiB): 64.00
        Read Look-Ahead: Enabled
        Write Cache: Enabled
        SMART Status: Good
        ATA Security Information: Supported, Frozen
        Zoned Device Type: Not a Zoned Device
        Firmware Download Support: Immediate, Segmented
        Specifications Supported:
                ACS-2
                ATA8-ACS
                ATA/ATAPI-7
                ATA/ATAPI-6
                ATA/ATAPI-5
                ATA/ATAPI-4
                SATA 3.1
                SATA 3.0
                SATA 2.6
                SATA 2.5
                SATA II: Extensions
                SATA 1.0a
        Features Supported:
                NCQ
                HPA
                Power Management
                Security
                SMART
                DCO
                48bit Address
                APM
                GPL
                Free-fall Control
                Write-Read-Verify

SATA SSD Device Information:

SeaChest_Firmware -d PD2 -i
===============================================================================
 SeaChest - Seagate drive utilities
 Copyright (c) 2014-2018 Seagate Technology LLC and/or its Affiliates, All Rights Reserved
===============================================================================
        Model Number: ST120FP0021
        Serial Number: PQ57011BD
        Firmware Revision: B770
        World Wide Name: 5000C501005A16633
        Drive Capacity (GB/GiB): 120.03/111.79
        Native Drive Capacity (GB/GiB): 120.03/111.79
        Temperature Data:
                Current Temperature (C): 26
                Highest Temperature (C): 0
                Lowest Temperature (C): 17
        Humidity Data:
                Current Humidity (%): Not Reported
                Highest Humidity (%): Not Reported
                Lowest Humidity (%): Not Reported
        Power On Time:  2 days 23 hours
        Power On Hours: 71.00
        MaxLBA: 234441647
        Native MaxLBA: 234441647
        Logical Sector Size (B): 512
        Physical Sector Size (B): 4096
        Sector Alignment: 0
        Rotation Rate (RPM): SSD
        Form Factor (inch): 2.5
        Last DST information:
                Not supported
        Interface speed:
                Max Speed (Gb/s): 6.0
                Negotiated Speed (Gb/s): 3.0
        Annualized Workload Rate (TB/yr): 299.80
        Total Bytes Read (TB): 2.35
        Total Bytes Written (GB): 90.19
        Drive Reported Utilization (%): Not Reported
        Encryption Support: Not Supported
        Cache Size (MiB): Not Reported
        Percentage Used Endurance Indicator (%): 0.00000
        Read Look-Ahead: Enabled
        Write Cache: Enabled
        SMART Status: Good
        ATA Security Information: Supported, Frozen
        Zoned Device Type: Not a Zoned Device
        Firmware Download Support: Immediate, Segmented
        Specifications Supported:
                ATA8-ACS
                ATA/ATAPI-7
                ATA/ATAPI-6
                ATA/ATAPI-5
                ATA/ATAPI-4
                SATA 3.0
        Features Supported:
                Sanitize
                NCQ
                HPA
                Power Management
                Security
                SMART
                48bit Address
                GPL
                TRIM

SAS HDD Device Information:

SeaChest_Firmware -i -d PD0
===============================================================================
 SeaChest - Seagate drive utilities
 Copyright (c) 2014-2018 Seagate Technology LLC and/or its Affiliates, All Rights Reserved
===============================================================================
        Model Number: ST4000NM0043
        Serial Number: Z1QZ04KVG
        Firmware Revision: 0004
        World Wide Name: 500Q0C5005594AEFB
        Copyright: Copyright (c) 2014 Seagate All rights reserved
        Drive Capacity (TB/TiB): 4.00/3.64
        Temperature Data:
                Current Temperature (C): 28
                Highest Temperature (C): Not Reported
                Lowest Temperature (C): Not Reported
        Humidity Data:
                Current Humidity (%): Not Reported
                Highest Humidity (%): Not Reported
                Lowest Humidity (%): Not Reported
        Power On Time:  61 days 11 hours 14 minutes
        Power On Hours: 1475.23
        MaxLBA: 7814037167
        Native MaxLBA: Not Reported
        Logical Sector Size (B): 512
        Physical Sector Size (B): 512
        Sector Alignment: 0
        Rotation Rate (RPM): 7200
        Form Factor (inch): 3.5
        Last DST information:
                Time since last DST (hours): 548.23
                DST Status/Result: 0x0
                DST Test run: 0x1
        Interface speed:
                Port 0 (Current Port)
                        Max Speed (GB/s): 6.0
                        Negotiated Speed (Gb/s): 3.0
                Port 1
                        Max Speed (GB/s): 6.0
                        Negotiated Speed (Gb/s): Not Reported
        Annualized Workload Rate (TB/yr): 0.02
        Total Bytes Read (GB): 2.27
        Total Bytes Written (GB): 2.39
        Drive Reported Utilization (%): Not Reported
        Encryption Support: Self Encrypting
        Cache Size (MiB): Not Reported
        Read Look-Ahead: Enabled
        Write Cache: Enabled
        SMART Status: Good
        ATA Security Information: Not Supported
        Zoned Device Type: Not a Zoned Device
        Firmware Download Support: Immediate
        Specifications Supported:
                SPC-4
        Features Supported:
                EPC
                TCG
                Self Test
                Informational Exceptions
                Format Unit
                Sanitize

SAS SSD: Device Information

SeaChest_Firmware -d PD3 -i
===============================================================================
 SeaChest - Seagate drive utilities
 Copyright (c) 2014-2018 Seagate Technology LLC and/or its Affiliates, All Rights Reserved
===============================================================================
        Model Number: ST400FM0053
        Serial Number: P3QF13026
        Firmware Revision: 0006
        World Wide Name: 5000QC50069010B4B
        Copyright: Copyright (c) 2014 Seagate All rights reserved -
        Drive Capacity (GB/GiB): 400.09/372.61
        Temperature Data:
                Current Temperature (C): 34
                Highest Temperature (C): Not Reported
                Lowest Temperature (C): Not Reported
        Humidity Data:
                Current Humidity (%): Not Reported
                Highest Humidity (%): Not Reported
                Lowest Humidity (%): Not Reported
        Power On Time:  30 days 21 hours 29 minutes
        Power On Hours: 741.48
        MaxLBA: 781422767
        Native MaxLBA: Not Reported
        Logical Sector Size (B): 512
        Physical Sector Size (B): 4096
        Sector Alignment: 0
        Rotation Rate (RPM): SSD
        Form Factor (inch): 2.5
        Last DST information:
                Time since last DST (hours): 434.48
                DST Status/Result: 0x0
                DST Test run: 0x1
        Interface speed:
                Port 0 (Current Port)
                        Max Speed (GB/s): 12.0
                        Negotiated Speed (Gb/s): 3.0
                Port 1
                        Max Speed (GB/s): 12.0
                        Negotiated Speed (Gb/s): Not Reported
        Annualized Workload Rate (TB/yr): 9.48
        Total Bytes Read (GB): 24.62
        Total Bytes Written (GB): 837.41
        Drive Reported Utilization (%): Not Reported
        Encryption Support: Not Supported
        Cache Size (MiB): Not Reported
        Percentage Used Endurance Indicator (%): 1.00000
        Read Look-Ahead: Enabled
        Write Cache: Enabled
        SMART Status: Good
        ATA Security Information: Not Supported
        Zoned Device Type: Not a Zoned Device
        Firmware Download Support: Immediate, Segmented, Deferred
        Specifications Supported:
                SPC-4
        Features Supported:
                EPC
                Power Comsumption
                UNMAP
                Self Test
                Informational Exceptions
                Format Unit
                Sanitize

===============
Version History - SeaChest_Firmware
===============
v0.0.1  22-Mar-2016  1_9_1 libraries.  SeaChest_Firmware Windows, initial beta
                     test release.  Branched from SeaChest_Basics v1.1.0.  Adds
                     firmware download batch modes by model number and various
                     firmware revision checks.
v0.0.2  19-May-2016  1_9_2 libraries fixed scan information from ATAPI devices.
                     Fixed a bug where we could accidentally clear some stored
                     identify data from the device structure. Fixed continuing
                     on when there was a permission denied error opening a
                     drive.
v1.0.0  15-Jun-2016  1_9_3 libraries fixed issues with ATA secure erase
                     commands. Fixed bugs with --modelMatch and --onlyFW
                     filters.
v1.1.0  06-Jul-2016  1_10_0 libraries add --forceATA and --forceSCSI.
v1.1.0  14-Jul-2016  1_10_1 libraries adds SMART and power management
                     functions, format polling, endianess detection, buffer
                     size fixes, SAS device statistics, Win32 IOCTL
                     pass-through fix on Win8 and higher.
v2.0.3  16-Aug-2016  Adds --fwdlInfo, --activateFW, --fwdlConfig and
                     --fwdlSegSize.  Add user defined configuration
                     files.
v2.0.4  23-Aug-2016  Adds --calculateFileHash.
v2.1.0  01-Sep-2016  1_11_1 libraries updates to various printed message,
                     minor bug fixes. Fixed --SATInfo command. After firmware
                     download messages improved. Logic to exclude using both
                     --fwdlConfig and --downloadFW at the same time.
v2.1.0  21-Sep-2016  1_11_2 libraries updates adds --forceATADMA, --forceATAPIO
                     and --forceATAUDMA  (SATA Only).
v2.2.0  10-Oct-2016  1_11_4 libraries updates. Support for multiple devices.
v2.2.0  25-Oct-2016  1_11_5 libraries updates improved LaCie  detection, adds
                     SAT Vendor ID, SAT Product ID, and SAT Product Revision to
                     the -i --SATInfo output.
v2.2.2  27-Oct-2016  1_11_6 libraries updates WWN detection.  Added
                     --enableLegacyUSBPassthrough
v2.2.2  03-Nov-2016  1_11_7 libraries fixed issue with SAS EPC power mode
                     settings.
v2.2.2  13-Dec-2016  1_11_10 libraries fixes a problem when using maxLBA without
                     the corresponding command range option, SAS power mode
                     setting, and Sanitize erase patterns.
v2.3.0  23-Feb-2017  1_13_0 libraries adds support for SAS 12.0Gb/s and
                     22.5Gb/s physical bus speeds, support for double buffered
                     passthrough IOCTLs. Add --fwdlDryRun. New -F, --scanFlags
                     [options: ignoreCSMI allowDuplicates] for Windows tools.
                     Add CSMI support to all Windows version tools.
v2.3.0  06-Mar-2017  1_13_2 libraries adds Enhanced device information output
                     for SAS features.
v2.3.2  09-Mar-2017  Fixes to config file processing.
v2.3.3  12-Apr-2017  1_13_4 libraries. Fixes issue where tool was not
                     defaulting to segmented download if not specified.  Adds
                     several new return exit codes to help manage scripts using
                     configuration files.
v2.3.4  10-May-2017  1_13_4 libraries. Fixes issue where where --fwdlInfo
                     command was sometimes missing segmented on SAS products.
v2.4.0  14-Jun-2017  1_15_0 libraries adds bug fix malformed command line
                     should exit with code = 1; added detection of parallel ATA
                     and SCSI speeds; temperature data on ATA now uses the
                     values from the SCT status log or device statistics log.
                     Bug fix where the "-d all" was not filtering out csmi
                     drives like it is supposed to causing duplicate drives to
                     show up.  Adds the child drive matching options
                     --childModelMatch, --childOnlyFW, and --childNewFW.
v2.5.0  14-Jul-2017  1_16_1 libraries adds support for ATA drives that have the
                     Sense Data Reporting feature enabled, changes to how we
                     interpret the completion status from the drive, new Sense
                     Data ASC, ASCQ definitions from SPC5. Adds --Scan (or -S,
                     note the capital S) aggressive system scan.
v2.5.0  27-Jul-2017  1_16_2 libraries enhances Seagate brand detection.
v2.5.0  19-Sep-2017  1_16_4 libraries fixes SCSI "--progress format", added
                     reading remanufacture time for SAS when the drive reports
                     a time, fixed SAS --abortDST.
v2.5.0  25-Sep-2017  1_17_0 libraries adds improved SATA device discovery on
                     SAS adapters, added NVMe read, write & Flush commands.
v2.5.1  10-Oct-2017  1_17_1 libraries adds Better handling of NVMe as a SCSI
                     device, SAT library strings, and fixes to Read-Buffer
                     error history (ISL). Updated copyright notice, invalid
                     command line options now only display an error instead of
                     long help. Added option to specify a buffer ID or FW slot,
                     file name added to the output of --showFileHash. Added
                     --firmwareSlot and --fwBufferID.
v2.5.1  12-Oct-2017  1_17_3 libraries improves Fast-Format compatibility on SAS.
v2.5.2  26-Oct-2017  1_17_5 libraries fixes SATA drive discovery behind HBAs
                     that don't show as SATA and don't support the SAT VPD
                     page; added Automatic fallback to 12byte CDBs during
                     initial device discovery;  integrated fixes for SAS
                     firmware download and fixes for SAS LongDST time
                     calculation; added detection of TCG Pyrite and Opalite
                     drives.
v2.5.2  31-Oct-2017  1_17_6 libraries adds ATA Security compatibility with SATL
                     on some LSI adapters, corrects firmware download issue
                     under Windows 10 API.
v2.5.2  02-Nov-2017  1_17_7 libraries fixes Long DST time on SCSI/SAS products.
v2.5.2  19-Apr-2018  1_18_0 libraries improves device detection of CD-ROM and
                     USB flash drives, support for early 90's PATA drives that
                     don't support LBA mode, bug fix where the last digit of
                     the SCSI Unit Serial Number was being dropped, additional
                     logic for deferred download completion status. --scan
                     --onlySeagate for just Seagate drives in a large system,
                     Long Drive Self Test Time in the -i output, write protect
                     status has been added for SCSI and NVMe in the -i output,
                     IDD enhancements for SAS, IDD enhancements to allow
                     captive mode on SATA, added USB Hacks to better support
                     some odd-ball USB devices and prevent crashes and improve
                     performance for some operations on them by issuing test
                     unit ready commands when something fails during device
                     discovery, automatic fall back to SAT 10 byte commands
                     during device discovery to help work with some USB
                     devices, some Legacy SCSI support enhancements (partially
                     from USB hacks development), enhanced SD to SG mapping in
                     Linux.
v2.5.4  21-Sep-2018  1_18_2 libraries Added in reading os-release PRETTY_NAME
                     field to get the OS name under linux; NVMe enabled;  fixed
                     a bug in the ATA activate FW command; added in reading ID
                     Data log and Device statistics logs page 0 to check the
                     list of supported pages; fixed a bug in the loop used to
                     read mode pages for -i information on SAS; IDD SAS
                     improvements; fixed a bug in DST & Clean with ATA drives
                     behind SCSI controllers. Fix for --modelMatch that have
                     spaces in the name. Added additional information to the
                     banner and -V data to show support levels. Add general
                     support for NVMe and NVMe specific identify data to "-i"
                     command. Add --allowFlexibleFWDLAPIUse.
v2.5.4  18-Oct-2018  1_18_3 libraries Added NVMe generic read command support.

=======================================
About SeaChest Command Line Diagnostics
=======================================
Seagate offers both graphical user interface (GUI) and command line interface
(CLI) diagnostic tools for our storage devices.  SeaTools for Windows and
SeaTools Bootable for end users are the two most popular GUI tools.  These
tools support 15 languages.

SeaChest diagnostics are command line utilities which are available for expert
users.  These command line tools assume the user is knowledgeable about running
software from the operating system command prompt.  CLI tools are in the
English language only and use "command line arguments" to define the various
tasks and specific devices.  SeaChest diagnostics are available for both Linux
and Windows environments.

Linux versions of SeaChest tools are available as stand alone 32 or 64-bit
executables you can copy to your own system.  Windows OS versions of SeaChest
diagnostics are installed through a typical setup wizard and can be removed via
the Control Panel.

In addition, Seagate offers a tool to build a bootable USB SeaChest flash drive
which boots to a 32-bit Linux command prompt.  This is a Windows executable
file which formats a USB Flash drive you provide.  It copies over all the files
needed to use it as a bootable device for the SeaChest diagnostic software.
All data on the USB Flash drive will be erased so be sure to protect any
valuable files.

Technical Support for SeaChest drive utilities is not available.  If you have
the time to send us some feedback about this software, especially if you notice
something we should fix or improve, we would greatly appreciate hearing from
you.  To report your comments and suggestions, please use this email
seaboard@seagate.com.  Please let us know the name and version of the tool you
are using.

SeaChest drive utilities support SATA, SAS and USB interface devices.

SeaChest Basics - Contains the most important tests and tools.

Other SeaChest "break out" utilities are available and listed below which offer
more in-depth functionality in specific areas. These are:

SeaChest Configure - Tools to control various settings on the drives are
brought together into this one tool.  Typical commands, for example, include
Write Cache and Read Lookahead Cache enable or disable.

SeaChest Erase - The focus is on data erasure.  There are many different
choices for erasing data from simple boot track erase to full cryptographic
erasure (when supported).  Be sure to back up important data before using this
tool.  Seagate is not responsible for lost user data.  This tool only works on
Seagate drives.

SeaChest Firmware - Seagate products are run by firmware.  Having the latest
firmware can improve performance and or reliability of your product.  Seagate
recommends applying new firmware to enhance the performance and or reliability
of your drive.  Most products may see one or two firmware updates within the
early life of the product.

SeaChest Format - Storage products which utilize the SAS, SCSI or Fibre
Channel interfaces are able to perform a full low-level media format in the
field.  The SCSI Format Unit command offers many specialty options to
accommodate a variety of conditions and to fine tune the procedure.  This
complex command deserves its own "break out" utility.

SeaChest GenericTests - Read Tests are the original disk drive diagnostic which
is to just read every sector on the drive, sequentially.  This tool offers
several common read tests which can be defined by either time or range.  In
addition, the Long Generic test has the ability to repair problem sectors,
possibly eliminating an unnecessary drive return.

SeaChest Info - Historical generic activity logs (like total bytes written and
power on hours) and performance logs (like temperature) are available for
analytical review.  Identification and inquiry data stored on the drive is also
provided.  A view of SMART and device statistics is available when supported by
the drive.

SeaChest PowerChoice - Seagate disk drives offer a multitude of options to
manage power.  This tool manipulates the various power modes.

SeaChest Security - Various settings are available on modern Seagate disk
drives which may be locked and unlocked.  These settings may interact with the
operating systems and systems BIOS.  Options also include cryptographic erase
for Self-Encrypting Drives (SED).

SeaChest SMART - This tool provides a closer look at the collected SMART
attributes data.  SMART stands for Self-Monitoring, Analysis and Reporting
Technology.  Short Drive Self Test is included as one of the standard SMART
commands. In addition, the DST & Clean test has the ability to repair problem
sectors, possibly eliminating an unnecessary drive return.

=================================
Support and Open Source Statement
=================================
SeaTools for Windows is available to download firmware to SAS drives, provided
they are not obscured by RAID controllers.

Seagate offers technical support for disk drive installation.  If you have any
questions related to Seagate products and technologies, feel free to submit
your request on our web site. See the web site for a list of world-wide
telephone numbers.

Seagate Support:
http://www.seagate.com/support-home/
Contact Us:
http://www.seagate.com/contacts/

Please report bugs/suggestions to seaboard@seagate.com. Include the output of
--version information in the email. See the user guide section 'General Usage
Hints' for information about saving output to a log file.

This software uses open source packages obtained with permission from the
relevant parties. For a complete list of open source components, sources and
licenses, please see our Linux USB Boot Maker Utility FAQ for additional
information.

This Windows version of SeaChest uses an open source project named wingetopt,
license shown below.

SeaChest Utilities use libraries from the opensea source code projects.  These
projects are maintained at http://github.com/seagate.
The libraries in use are opensea-common, opensea-transport and
opensea-operations. These libraries are available under the Mozilla Public
License 2.0, license shown below.

The newest online version of the SeaChest Utilities documentation, open source
usage and acknowledgement licenses can be found at:
http://support.seagate.com/seachest/SeaChest_Combo_UserGuides.html

SeaChest_Firmware uses two open source projects named mbedtls and zlib.h,
licenses shown below.

Copyright (c) 2014-2018 Seagate Technology LLC and/or its Affiliates, All Rights Reserved
======================================================================

                        END USER LICENSE AGREEMENT
                            FOR SEAGATE SOFTWARE


PLEASE READ THIS END USER LICENSE AGREEMENT ("EULA") CAREFULLY.  BY CLICKING
"I AGREE" OR TAKING ANY STEP TO DOWNLOAD, SET-UP, INSTALL OR USE ALL OR ANY
PORTION OF THIS PRODUCT (INCLUDING, BUT NOT LIMITED TO, THE SOFTWARE AND
ASSOCIATED FILES (THE "SOFTWARE"), HARDWARE ("HARDWARE"), DISK (S), OR OTHER
MEDIA) (COLLECTIVELY, THE "PRODUCT") YOU AND YOUR COMPANY ACCEPT ALL THE
TERMS AND CONDITIONS OF THIS EULA.  IF YOU ACQUIRE THIS PRODUCT FOR YOUR
COMPANY’S USE, YOU REPRESENT THAT YOU ARE AN AUTHORIZED REPRESENTATIVE WHO
HAS THE AUTHORITY TO LEGALLY BIND YOUR COMPANY TO THIS EULA.  IF YOU DO NOT
AGREE, DO NOT CLICK "I AGREE" AND DO NOT DOWNLOAD, SET-UP, INSTALL OR USE THE
SOFTWARE.


1.  Ownership.  This EULA applies to the Software and Products of Seagate
Technology LLC and the affiliates controlled by, under common control with,
or controlling Seagate Technology LLC, including but not limited to
affiliates operating under the LaCie name or brand, (collectively, "Seagate",
"we", "us", "our").  Seagate and its suppliers own all right, title, and
interest in and to the Software, including all intellectual property rights
therein.  The Software is licensed, not sold.  The structure, organization,
and code of the Software are the valuable trade secrets and confidential
information of Seagate and its suppliers.  The Software is protected by
copyright and other intellectual property laws and treaties, including,
without limitation, the copyright laws of the United States and other
countries. The term "Software" does not refer to or include "Third-Party
Software".  "Third-Party Software" means certain software licensed by Seagate
from third parties that may be provided with the specific version of Software
that you have licensed.  The Third-Party Software is generally not governed
by the terms set forth below but is subject to different terms and conditions
imposed by the licensors of such Third-Party Software.  The terms of your use
of the Third-Party Software are subject to and governed by the respective
license terms, except that this Section 1 and Sections 5 and 6 of this
Agreement also govern your use of the Third-Party Software.  You may identify
and view the relevant licenses and/or notices for such Third-Party Software
for the Software you have received pursuant to this EULA at
http://www.seagate.com/support/by-topic/downloads/ , or at
http://www.lacie.com/support/ for LaCie branded product. You agree to comply
with the terms and conditions contained in all such Third-Party Software
licenses with respect to the applicable Third-Party Software. Where
applicable, the URLs for sites where you may obtain source code for the Third
Party Software can be found at
http://www.seagate.com/support/by-topic/downloads/, or at
http://www.lacie.com/support/ for LaCie branded product.

2.  Product License.  Subject to your compliance with the terms of this EULA,
Seagate grants you a personal, non-exclusive, non-transferable, limited
license to install and use one (1) copy of the Software on one (1) device
residing on your premises, internally and only for the purposes described in
the associated documentation. Use of some third party software included on
the media provided with the Product may be subject to terms and conditions of
a separate license agreement; this license agreement may be contained in a
"Read Me" file located on the media that accompanies that Product.  The
Software includes components that enable you to link to and use certain
services provided by third parties ("Third Party Services").  Your use of the
Third Party Services is subject to your agreement with the applicable third
party service provider.  Except as expressly stated herein, this EULA does
not grant you any intellectual property rights in the Product. Seagate and
its suppliers reserve all rights not expressly granted to you.  There are no
implied rights.

2.1     Software.  You are also permitted to make a single copy of the
Software strictly for backup and disaster recovery purposes.  You may not
alter or modify the Software or create a new installer for the Software.  The
Software is licensed and distributed by Seagate for use with its storage
products only, and may not be used with non-Seagate storage product.

3.  Restrictions.  You are not licensed to do any of the following:
        a.      Create derivative works based on the Product or any part or
                component thereof, including, but not limited to, the
                Software;

        b.      Reproduce the Product, in whole or in part;

        c.      Except as expressly authorized by Section 11 below, sell,
                assign, license, disclose, or otherwise transfer or make
                available the Product, in whole or in part, to any third
                party;

        d.      Alter, translate, decompile, or attempt to reverse engineer
                the Product or any part or component thereof, except and only
                to the extent that such activity is expressly permitted by
                applicable law notwithstanding this contractual prohibition;

        e.      Use the Product to provide services to third parties;

        f.      Take any actions that would cause the Software to become
                subject to any open source license agreement if it is not
                already subject to such an agreement; and

        g.      Remove or alter any proprietary notices or marks on the
                Product.

4.  Updates.  If you receive an update or an upgrade to, or a new version of,
any Software ("Update") you must possess a valid license to the previous
version in order to use the Update.  All Updates provided to you shall be
subject to the terms and conditions of this EULA.  If you receive an Update,
you may continue to use the previous version(s) of the Software in your
possession, custody or control.  Seagate shall have no obligation to support
the previous versions of the Software upon availability of an Update. Seagate
has no obligation to provide support, maintenance, Updates, or modifications
under this EULA.

5.  NO WARRANTY.  THE PRODUCT AND THE THIRD-PARTY SOFTWARE ARE OFFERED ON AN
"AS-IS" BASIS AND NO WARRANTY, EITHER EXPRESS OR IMPLIED, IS GIVEN.  SEAGATE
AND ITS SUPPLIERS EXPRESSLY DISCLAIM ALL WARRANTIES OF ANY KIND, WHETHER
STATUTORY, EXPRESS OR IMPLIED, INCLUDING, BUT NOT LIMITED TO, IMPLIED
WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
NON-INFRINGEMENT.  SEAGATE DOES NOT PROVIDE THE THIRD PARTY SERVICES AND
MAKES NO WARRANTIES WITH RESPECT TO THE THIRD PARTY SERVICES.  YOUR USE OF
THE THIRD PARTY SERVICES IS AT YOUR RISK.

6.  EXCLUSION OF INCIDENTAL, CONSEQUENTIAL, AND CERTAIN OTHER DAMAGES.  TO
THE MAXIMUM EXTENT PERMITTED BY APPLICABLE LAW, IN NO EVENT SHALL SEAGATE OR
ITS LICENSORS OR SUPPLIERS BE LIABLE FOR ANY SPECIAL, INCIDENTAL, PUNITIVE,
INDIRECT, OR CONSEQUENTIAL DAMAGES WHATSOEVER (INCLUDING, BUT NOT LIMITED TO,
DAMAGES FOR LOSS OF PROFITS OR CONFIDENTIAL OR OTHER INFORMATION, FOR
BUSINESS INTERRUPTION, FOR PERSONAL INJURY, FOR LOSS OF PRIVACY, FOR FAILURE
TO MEET ANY DUTY INCLUDING OF GOOD FAITH OR REASONABLE CARE, FOR NEGLIGENCE,
AND FOR ANY OTHER PECUNIARY OR OTHER LOSS WHATSOEVER) ARISING OUT OF OR IN
ANY WAY RELATED TO THE USE OF OR INABILITY TO USE THE PRODUCT OR ANY PART OR
COMPONENT THEREOF OR RELATED SERVICE OR ANY THIRD PARTY SERVICES, OR
OTHERWISE UNDER OR IN CONNECTION WITH ANY PROVISION OF THE EULA, EVEN IN THE
EVENT OF THE FAULT, TORT (INCLUDING NEGLIGENCE), MISREPRESENTATION, STRICT
LIABILITY, BREACH OF CONTRACT, OR BREACH OF WARRANTY OF SEAGATE OR ITS
LICENSORS OR SUPPLIERS, AND EVEN IF SEAGATE OR ITS LICENSOR OR SUPPLIER HAS
BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES AND NOTWITHSTANDING ANY
FAILURE OF THE ESSENTIAL PURPOSE OF THIS AGREEMENT OR ANY REMEDY.

7.  LIMITATION OF LIABILITY.  NOTWITHSTANDING ANY DAMAGES THAT YOU MIGHT
INCUR FOR ANY REASON WHATSOEVER, THE ENTIRE LIABILITY OF SEAGATE UNDER ANY
PROVISION OF THIS EULA AND YOUR EXCLUSIVE REMEDY HEREUNDER SHALL BE LIMITED
TO, AND IN NO EVENT WILL SEAGATE'S TOTAL CUMULATIVE DAMAGES EXCEED, THE FEES
PAID BY THE LICENSEE TO SEAGATE FOR THE PRODUCT.  ADDITIONALLY, IN NO EVENT
SHALL SEAGATE'S LICENSORS OR SUPPLIERS BE LIABLE FOR ANY DAMAGES OF ANY KIND.

8.  Privacy.  Seagate’s collection, use and disclosure of personally
identifiable information in connection with your use of the Product is
governed by Seagate’s Privacy Policy which is located at
http://www.seagate.com/legal-privacy/privacy-policy/As further described in
Seagate’s Privacy Policy, certain Products may include a Product dashboard
which allows users to manage Product settings, including but not limited to
use of anonymous statistical usage data in connection with personally
identifiable information. You agree to Seagate’s collection, use, and
disclosure of your data in accordance with the Product dashboard settings
selected by you for the Product, or in the case of transfer as described in
Section 11, you agree to the settings selected by the prior licensee unless
or until you make changes to the settings.

9.  Indemnification.  By accepting the EULA, you agree to indemnify and
otherwise hold harmless Seagate, its officers, employees, agents,
subsidiaries, affiliates, and other partners from any direct, indirect,
incidental, special, consequential or exemplary damages arising out of,
relating to, or resulting from your use of the Product or any other matter
relating to the Product, including, without limitation, use of any of the
Third Party Services.

10.  International Trade Compliance.  The Software and any related technical
data made available for download under this EULA are subject to the customs
and export control laws and regulations of the United States ("U.S.") and may
also be subject to the customs and export laws and regulations of the country
in which the download is contemplated.  Further, under U.S. law, the Software
and any related technical data made available for download under this EULA
may not be sold, leased or otherwise transferred to restricted countries, or
used by a restricted end-user (as determined on any one of the U.S.
government restricted parties lists, found at
http://www.bis.doc.gov/complianceandenforcement/liststocheck.htm) or an
end-user engaged in activities related to weapons of mass destruction
including, without limitation, activities related to designing, developing,
producing or using nuclear weapons, materials, or facilities, missiles or
supporting missile projects, or chemical or biological weapons.  You
acknowledge that you are not a citizen, national, or resident of, and are not
under control of the governments of Cuba, Iran, North Korea, Sudan or Syria;
are not otherwise a restricted end-user as defined by U.S. export control
laws; and are not engaged in proliferation activities.  Further, you
acknowledge that you will not download or otherwise export or re-export the
Software or any related technical data directly or indirectly to the
above-mentioned countries or to citizens, nationals, or residents of those
countries, or to any other restricted end user or for any restricted end-use.

11.  General.  This EULA between Licensee and Seagate is governed by and
construed in accordance with the laws of the State of California without
regard to conflict of laws principles.  The EULA constitutes the entire
agreement between Seagate and you relating to the Product and governs your
use of the Product, superseding any prior agreement between you and Seagate
relating to the subject matter hereof.  If any provision of this EULA is held
by a court of competent jurisdiction to be contrary to law, such provision
will be changed and interpreted so as to best accomplish the objectives of
the original provision to the fullest extent allowed by law and the remaining
provisions of the EULA will remain in force and effect.  The Product and any
related technical data are provided with restricted rights.  Use,
duplication, or disclosure by the U.S. government is subject to the
restrictions as set forth in subparagraph (c)(1)(iii) of DFARS 252.227-7013
(The Rights in Technical Data and Computer Product) or subparagraphs (c)(1)
and (2) of 48 CFR 52.227-19 (Commercial Computer Product – Restricted
Rights), as applicable.  The manufacturer is Seagate.  You may not transfer
or assign this EULA or any rights under this EULA, except that you may make a
one-time, permanent transfer of this EULA and the Software to another end
user, provided that (i) you do not retain any copies of the Software, the
Hardware, the media and printed materials, Upgrades (if any), and this EULA,
and (ii) prior to the transfer, the end user receiving this EULA and the
Software agrees to all the EULA terms.  Any attempted assignment in violation
of this Section is void.  Seagate, the Seagate logo, and other Seagate names
and logos are the trademarks of Seagate.

5.4.2016

===========================================================================

GNU LESSER GENERAL PUBLIC LICENSE

Version 3, 29 June 2007

Copyright (c) 2007 Free Software Foundation, Inc. <http://fsf.org/>

Everyone is permitted to copy and distribute verbatim copies of this license
document, but changing it is not allowed.

This version of the GNU Lesser General Public License incorporates the terms
and conditions of version 3 of the GNU General Public License, supplemented
by the additional permissions listed below.

0. Additional Definitions.

As used herein, "this License" refers to version 3 of the GNU Lesser General
Public License, and the "GNU GPL" refers to version 3 of the GNU General
Public License.

"The Library" refers to a covered work governed by this License, other than
an Application or a Combined Work as defined below.

An "Application" is any work that makes use of an interface provided by the
Library, but which is not otherwise based on the Library. Defining a subclass
of a class defined by the Library is deemed a mode of using an interface
provided by the Library.

A "Combined Work" is a work produced by combining or linking an Application
with the Library. The particular version of the Library with which the
Combined Work was made is also called the "Linked Version".

The "Minimal Corresponding Source" for a Combined Work means the
Corresponding Source for the Combined Work, excluding any source code for
portions of the Combined Work that, considered in isolation, are based on the
Application, and not on the Linked Version.

The "Corresponding Application Code" for a Combined Work means the object
code and/or source code for the Application, including any data and utility
programs needed for reproducing the Combined Work from the Application, but
excluding the System Libraries of the Combined Work.

1. Exception to Section 3 of the GNU GPL.

You may convey a covered work under sections 3 and 4 of this License without
being bound by section 3 of the GNU GPL.

2. Conveying Modified Versions.

If you modify a copy of the Library, and, in your modifications, a facility
refers to a function or data to be supplied by an Application that uses the
facility (other than as an argument passed when the facility is invoked),
then you may convey a copy of the modified version:

* a) under this License, provided that you make a good faith effort to ensure
that, in the event an Application does not supply the function or data, the
facility still operates, and performs whatever part of its purpose remains
meaningful, or

* b) under the GNU GPL, with none of the additional permissions of this
License applicable to that copy.

3. Object Code Incorporating Material from Library Header Files.

The object code form of an Application may incorporate material from a header
file that is part of the Library. You may convey such object code under terms
of your choice, provided that, if the incorporated material is not limited to
numerical parameters, data structure layouts and accessors, or small macros,
inline functions and templates (ten or fewer lines in length), you do both of
the following:

* a) Give prominent notice with each copy of the object code that the Library
is used in it and that the Library and its use are covered by this License.

* b) Accompany the object code with a copy of the GNU GPL and this license
document.

4. Combined Works.

You may convey a Combined Work under terms of your choice that, taken
together, effectively do not restrict modification of the portions of the
Library contained in the Combined Work and reverse engineering for debugging
such modifications, if you also do each of the following:

* a) Give prominent notice with each copy of the Combined Work that the
Library is used in it and that the Library and its use are covered by this
License.

* b) Accompany the Combined Work with a copy of the GNU GPL and this license
document.

* c) For a Combined Work that displays copyright notices during execution,
include the copyright notice for the Library among these notices, as well as
a reference directing the user to the copies of the GNU GPL and this license
document.

* d) Do one of the following:
  o 0) Convey the Minimal Corresponding Source under the terms of this
License, and the Corresponding Application Code in a form suitable for, and
under terms that permit, the user to recombine or relink the Application
with a modified version of the Linked Version to produce a modified
Combined Work, in the manner specified by section 6 of the GNU GPL for
conveying Corresponding Source.
  o 1) Use a suitable shared library mechanism for linking with the Library.
A suitable mechanism is one that (a) uses at run time a copy of the Library
already present on the user's computer system, and (b) will operate
properly with a modified version of the Library that is
interface-compatible with the Linked Version.

* e) Provide Installation Information, but only if you would otherwise be
required to provide such information under section 6 of the GNU GPL, and only
to the extent that such information is necessary to install and execute a
modified version of the Combined Work produced by recombining or relinking
the Application with a modified version of the Linked Version. (If you use
option 4d0, the Installation Information must accompany the Minimal
Corresponding Source and Corresponding Application Code. If you use option
4d1, you must provide the Installation Information in the manner specified by
section 6 of the GNU GPL for conveying Corresponding Source.)

5. Combined Libraries.

You may place library facilities that are a work based on the Library side by
side in a single library together with other library facilities that are not
Applications and are not covered by this License, and convey such a combined
library under terms of your choice, if you do both of the following:

* a) Accompany the combined library with a copy of the same work based on the
Library, uncombined with any other library facilities, conveyed under the
terms of this License.

* b) Give prominent notice with the combined library that part of it is a
work based on the Library, and explaining where to find the accompanying
uncombined form of the same work.

6. Revised Versions of the GNU Lesser General Public License.

The Free Software Foundation may publish revised and/or new versions of the
GNU Lesser General Public License from time to time. Such new versions will
be similar in spirit to the present version, but may differ in detail to
address new problems or concerns.

Each version is given a distinguishing version number. If the Library as you
received it specifies that a certain numbered version of the GNU Lesser
General Public License "or any later version" applies to it, you have the
option of following the terms and conditions either of that published version
or of any later version published by the Free Software Foundation. If the
Library as you received it does not specify a version number of the GNU
Lesser General Public License, you may choose any version of the GNU Lesser
General Public License ever published by the Free Software Foundation.

If the Library as you received it specifies that a proxy can decide whether
future versions of the GNU Lesser General Public License shall apply, that
proxy's public statement of acceptance of any version is permanent
authorization for you to choose that version for the Library.

===========================================================================
wingetopt - getopt library for Windows compilers

This library was created to allow compilation linux-based software on Windows.
http://en.wikipedia.org/wiki/Getopt  The sources were taken from MinGW-runtime
project.

AUTHORS: Todd C. Miller Todd.Miller@courtesan.com; The NetBSD Foundation, Inc.

LICENSE

Copyright (c) 2002 Todd C. Miller <Todd.Miller@courtesan.com>

Permission to use, copy, modify, and distribute this software for any purpose
with or without fee is hereby granted, provided that the above copyright notice
and this permission notice appear in all copies.

THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES WITH
REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF MERCHANTABILITY AND
FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY SPECIAL, DIRECT,
INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES WHATSOEVER RESULTING FROM
LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION OF CONTRACT, NEGLIGENCE OR
OTHER TORTIOUS ACTION, ARISING OUT OF OR IN CONNECTION WITH THE USE OR
PERFORMANCE OF THIS SOFTWARE.

Sponsored in part by the Defense Advanced Research Projects Agency (DARPA) and
Air Force Research Laboratory, Air Force Materiel Command, USAF, under
agreement number F39502-99-1-0512.

                 -------------------------------------

Copyright (c) 2000 The NetBSD Foundation, Inc.
All rights reserved.

This code is derived from software contributed to The NetBSD Foundation
by Dieter Baron and Thomas Klausner.

Redistribution and use in source and binary forms, with or without
modification, are permitted provided that the following conditions are met:
1. Redistributions of source code must retain the above copyright notice, this
   list of conditions and the following disclaimer.
2. Redistributions in binary form must reproduce the above copyright notice,
   this list of conditions and the following disclaimer in the documentation
   and/or other materials provided with the distribution.

THIS SOFTWARE IS PROVIDED BY THE NETBSD FOUNDATION, INC. AND CONTRIBUTORS "AS
IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
DISCLAIMED.  IN NO EVENT SHALL THE FOUNDATION OR CONTRIBUTORS BE LIABLE FOR ANY
DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
(INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
(INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

===========================================================================
mbedtls - An open source, portable, easy to use, readable and flexible SSL
library https://tls.mbed.org

Modifications: -added DES & 3DES CFB cipher encryption and decryption support

         Apache License
   Version 2.0, January 2004
http://www.apache.org/licenses/

TERMS AND CONDITIONS FOR USE, REPRODUCTION, AND DISTRIBUTION

1. Definitions.

"License" shall mean the terms and conditions for use, reproduction, and
distribution as defined by Sections 1 through 9 of this document.

"Licensor" shall mean the copyright owner or entity authorized by the copyright
owner that is granting the License.

"Legal Entity" shall mean the union of the acting entity and all other entities
that control, are controlled by, or are under common control with that entity.
For the purposes of this definition, "control" means (i) the power, direct or
indirect, to cause the direction or management of such entity, whether by
contract or otherwise, or (ii) ownership of fifty percent (50) or more of the
outstanding shares, or (iii) beneficial ownership of such entity.

"You" (or "Your") shall mean an individual or Legal Entity exercising
permissions granted by this License.

"Source" form shall mean the preferred form for making modifications, including
but not limited to software source code, documentation source,and configuration
files.

"Object" form shall mean any form resulting from mechanical transformation or
translation of a Source form, including but not limited to compiled object
code, generated documentation, and conversions to other media types.

"Work" shall mean the work of authorship, whether in Source or Object form,
made available under the License, as indicated by a copyright notice that is
included in or attached to the work (an example is provided in the Appendix
below).

"Derivative Works" shall mean any work, whether in Source or Object form, that
is based on (or derived from) the Work and for which the editorial revisions,
annotations, elaborations, or other modifications represent, as a whole, an
original work of authorship. For the purposes of this License, Derivative Works
shall not include works that remain separable from, or merely link (or bind by
name) to the interfaces of, the Work and Derivative Works thereof.

"Contribution" shall mean any work of authorship, including the original
version of the Work and any modifications or additions to that Work or
Derivative Works thereof, that is intentionally submitted to Licensor for
inclusion in the Work by the copyright owner or by an individual or Legal
Entity authorized to submit on behalf of the copyright owner. For the purposes
of this definition, "submitted" means any form of electronic, verbal, or
written communication sent to the Licensor or its representatives, including
but not limited to communication on electronic mailing lists, source code
control systems, and issue tracking systems that are managed by, or on behalf
of, the Licensor for the purpose of discussing and improving the Work, but
excluding communication that is conspicuously marked or otherwise designated in
writing by the copyright owner as "Not a Contribution."

"Contributor" shall mean Licensor and any individual or Legal Entity on behalf
of whom a Contribution has been received by Licensor and subsequently
incorporated within the Work.

2. Grant of Copyright License. Subject to the terms and conditions of this
License, each Contributor hereby grants to You a perpetual, worldwide,
non-exclusive, no-charge, royalty-free, irrevocable copyright license to
reproduce, prepare Derivative Works of, publicly display, publicly perform,
sublicense, and distribute the Work and such Derivative Works in Source or
Object form.

3. Grant of Patent License. Subject to the terms and conditions of this
License, each Contributor hereby grants to You a perpetual, worldwide,
non-exclusive, no-charge, royalty-free, irrevocable (except as stated in this
section) patent license to make, have made, use, offer to sell, sell, import,
and otherwise transfer the Work, where such license applies only to those
patent claims licensable by such Contributor that are necessarily infringed by
their Contribution(s) alone or by combination of their Contribution(s) with the
Work to which such Contribution(s) was submitted. If You institute patent
litigation against any entity (including a cross-claim or counterclaim in a
lawsuit) alleging that the Work or a Contribution incorporated within the Work
constitutes direct or contributory patent infringement, then any patent
licenses granted to You under this License for that Work shall terminate as of
the date such litigation is filed.

4. Redistribution. You may reproduce and distribute copies of the Work or
Derivative Works thereof in any medium, with or without modifications, and in
Source or Object form, provided that You meet the following conditions:

(a) You must give any other recipients of the Work or Derivative Works a copy
of this License; and

(b) You must cause any modified files to carry prominent notices stating that
You changed the files; and

(c) You must retain, in the Source form of any Derivative Works that You
distribute, all copyright, patent, trademark, and attribution notices from the
Source form of the Work, excluding those notices that do not pertain to any
part of the Derivative Works; and

(d) If the Work includes a "NOTICE" text file as part of its distribution, then
any Derivative Works that You distribute must include a readable copy of the
attribution notices contained within such NOTICE file, excluding those notices
that do not pertain to any part of the Derivative Works, in at least one of the
following places: within a NOTICE text file distributed as part of the
Derivative Works; within the Source form or documentation, if provided along
with the Derivative Works; or, within a display generated by the Derivative
Works, if and wherever such third-party notices normally appear. The contents
of the NOTICE file are for informational purposes only and do not modify the
License. You may add Your own attribution notices within Derivative Works that
You distribute, alongside or as an addendum to the NOTICE text from the Work,
provided that such additional attribution notices cannot be construed as
modifying the License.

You may add Your own copyright statement to Your modifications and may provide
additional or different license terms and conditions for use, reproduction, or
distribution of Your modifications, or for any such Derivative Works as a
whole, provided Your use, reproduction, and distribution of the Work otherwise
complies with the conditions stated in this License.

5. Submission of Contributions. Unless You explicitly state otherwise, any
Contribution intentionally submitted for inclusion in the Work by You to the
Licensor shall be under the terms and conditions of this License, without any
additional terms or conditions. Notwithstanding the above, nothing herein shall
supersede or modify the terms of any separate license agreement you may have
executed with Licensor regarding such Contributions.

6. Trademarks. This License does not grant permission to use the trade names,
trademarks, service marks, or product names of the Licensor, except as required
for reasonable and customary use in describing the origin of the Work and
reproducing the content of the NOTICE file.

7. Disclaimer of Warranty. Unless required by applicable law or agreed to in
writing, Licensor provides the Work (and each Contributor provides its
Contributions) on an "AS IS" BASIS, WITHOUT WARRANTIES OR CONDITIONS OF ANY
KIND, either express or implied, including, without limitation, any warranties
or conditions of TITLE, NON-INFRINGEMENT, MERCHANTABILITY, or FITNESS FOR A
PARTICULAR PURPOSE. You are solely responsible for determining the
appropriateness of using or redistributing the Work and assume any risks
associated with Your exercise of permissions under this License.

8. Limitation of Liability. In no event and under no legal theory, whether in
tort (including negligence), contract, or otherwise, unless required by
applicable law (such as deliberate and grossly negligent acts) or agreed to in
writing, shall any Contributor be liable to You for damages, including any
direct, indirect, special, incidental, or consequential damages of any
character arising as a result of this License or out of the use or inability to
use the Work (including but not limited to damages for loss of goodwill, work
stoppage, computer failure or malfunction, or any and all other commercial
damages or losses), even if such Contributor has been advised of the
possibility of such damages.

9. Accepting Warranty or Additional Liability. While redistributing the Work or
Derivative Works thereof, You may choose to offer, and charge a fee for,
acceptance of support, warranty, indemnity, or other liability obligations
and/or rights consistent with this License. However, in accepting such
obligations, You may act only on Your own behalf and on Your sole
responsibility, not on behalf of any other Contributor, and only if You agree
to indemnify, defend, and hold each Contributor harmless for any liability
incurred by, or claims asserted against, such Contributor by reason of your
accepting any such warranty or additional liability.

END OF TERMS AND CONDITIONS

APPENDIX: How to apply the Apache License to your work.

To apply the Apache License to your work, attach the following boilerplate
notice, with the fields enclosed by brackets "[]" replaced with your own
identifying information. (Don't include the brackets!) The text should be
enclosed in the appropriate comment syntax for the file format. We also
recommend that a file or class name and description of purpose be included on
the same "printed page" as the copyright notice for easier identification
within third-party archives.

Copyright [yyyy] [name of copyright owner]

Licensed under the Apache License, Version 2.0 (the "License"); you may not use
this file except in compliance with the License. You may obtain a copy of the
License at

http://www.apache.org/licenses/LICENSE-2.0

Unless required by applicable law or agreed to in writing, software distributed
under the License is distributed on an "AS IS" BASIS, WITHOUT WARRANTIES OR
CONDITIONS OF ANY KIND, either express or implied. See the License for the
specific language governing permissions and limitations under the License.

===========================================================================

zlib.h -- interface of the 'zlib' general purpose compression library version
1.2.8, April 28th, 2013

Copyright (C) 1995-2013 Jean-loup Gailly and Mark Adler

This software is provided 'as-is', without any express or implied warranty. In
no event will the authors be held liable for any damages arising from the use
of this software.

Permission is granted to anyone to use this software for any purpose, including
commercial applications, and to alter it and redistribute it freely, subject to
the following restrictions:

1. The origin of this software must not be misrepresented; you must not claim
that you wrote the original software. If you use this software in a product, an
acknowledgment in the product documentation would be appreciated but is not
required.

2. Altered source versions must be plainly marked as such, and must not be
misrepresented as being the original software.

3. This notice may not be removed or altered from any source distribution.

Jean-loup Gailly        Mark Adler jloup@gzip.org
madler@alumni.caltech.edu

======================================================================

SOURCE CODE files of the opensea open source project have been made available
to you under the Mozilla Public License 2.0 (MPL).  Mozilla is the custodian of
the Mozilla Public License ("MPL"), an open source/free software license.

https://www.mozilla.org/en-US/MPL/

Mozilla Public License Version 2.0
==================================

1. Definitions
--------------

1.1. "Contributor"
    means each individual or legal entity that creates, contributes to
    the creation of, or owns Covered Software.

1.2. "Contributor Version"
    means the combination of the Contributions of others (if any) used
    by a Contributor and that particular Contributor's Contribution.

1.3. "Contribution"
    means Covered Software of a particular Contributor.

1.4. "Covered Software"
    means Source Code Form to which the initial Contributor has attached
    the notice in Exhibit A, the Executable Form of such Source Code
    Form, and Modifications of such Source Code Form, in each case
    including portions thereof.

1.5. "Incompatible With Secondary Licenses"
    means

    (a) that the initial Contributor has attached the notice described
        in Exhibit B to the Covered Software; or

    (b) that the Covered Software was made available under the terms of
        version 1.1 or earlier of the License, but not also under the
        terms of a Secondary License.

1.6. "Executable Form"
    means any form of the work other than Source Code Form.

1.7. "Larger Work"
    means a work that combines Covered Software with other material, in
    a separate file or files, that is not Covered Software.

1.8. "License"
    means this document.

1.9. "Licensable"
    means having the right to grant, to the maximum extent possible,
    whether at the time of the initial grant or subsequently, any and
    all of the rights conveyed by this License.

1.10. "Modifications"
    means any of the following:

    (a) any file in Source Code Form that results from an addition to,
        deletion from, or modification of the contents of Covered
        Software; or

    (b) any new file in Source Code Form that contains any Covered
        Software.

1.11. "Patent Claims" of a Contributor
    means any patent claim(s), including without limitation, method,
    process, and apparatus claims, in any patent Licensable by such
    Contributor that would be infringed, but for the grant of the
    License, by the making, using, selling, offering for sale, having
    made, import, or transfer of either its Contributions or its
    Contributor Version.

1.12. "Secondary License"
    means either the GNU General Public License, Version 2.0, the GNU
    Lesser General Public License, Version 2.1, the GNU Affero General
    Public License, Version 3.0, or any later versions of those
    licenses.

1.13. "Source Code Form"
    means the form of the work preferred for making modifications.

1.14. "You" (or "Your")
    means an individual or a legal entity exercising rights under this
    License. For legal entities, "You" includes any entity that
    controls, is controlled by, or is under common control with You. For
    purposes of this definition, "control" means (a) the power, direct
    or indirect, to cause the direction or management of such entity,
    whether by contract or otherwise, or (b) ownership of more than
    fifty percent (50%) of the outstanding shares or beneficial
    ownership of such entity.

2. License Grants and Conditions
--------------------------------

2.1. Grants

Each Contributor hereby grants You a world-wide, royalty-free,
non-exclusive license:

(a) under intellectual property rights (other than patent or trademark)
    Licensable by such Contributor to use, reproduce, make available,
    modify, display, perform, distribute, and otherwise exploit its
    Contributions, either on an unmodified basis, with Modifications, or
    as part of a Larger Work; and

(b) under Patent Claims of such Contributor to make, use, sell, offer
    for sale, have made, import, and otherwise transfer either its
    Contributions or its Contributor Version.

2.2. Effective Date

The licenses granted in Section 2.1 with respect to any Contribution
become effective for each Contribution on the date the Contributor first
distributes such Contribution.

2.3. Limitations on Grant Scope

The licenses granted in this Section 2 are the only rights granted under
this License. No additional rights or licenses will be implied from the
distribution or licensing of Covered Software under this License.
Notwithstanding Section 2.1(b) above, no patent license is granted by a
Contributor:

(a) for any code that a Contributor has removed from Covered Software;
    or

(b) for infringements caused by: (i) Your and any other third party's
    modifications of Covered Software, or (ii) the combination of its
    Contributions with other software (except as part of its Contributor
    Version); or

(c) under Patent Claims infringed by Covered Software in the absence of
    its Contributions.

This License does not grant any rights in the trademarks, service marks,
or logos of any Contributor (except as may be necessary to comply with
the notice requirements in Section 3.4).

2.4. Subsequent Licenses

No Contributor makes additional grants as a result of Your choice to
distribute the Covered Software under a subsequent version of this
License (see Section 10.2) or under the terms of a Secondary License (if
permitted under the terms of Section 3.3).

2.5. Representation

Each Contributor represents that the Contributor believes its
Contributions are its original creation(s) or it has sufficient rights
to grant the rights to its Contributions conveyed by this License.

2.6. Fair Use

This License is not intended to limit any rights You have under
applicable copyright doctrines of fair use, fair dealing, or other
equivalents.

2.7. Conditions

Sections 3.1, 3.2, 3.3, and 3.4 are conditions of the licenses granted
in Section 2.1.

3. Responsibilities
-------------------

3.1. Distribution of Source Form

All distribution of Covered Software in Source Code Form, including any
Modifications that You create or to which You contribute, must be under
the terms of this License. You must inform recipients that the Source
Code Form of the Covered Software is governed by the terms of this
License, and how they can obtain a copy of this License. You may not
attempt to alter or restrict the recipients' rights in the Source Code
Form.

3.2. Distribution of Executable Form

If You distribute Covered Software in Executable Form then:

(a) such Covered Software must also be made available in Source Code
    Form, as described in Section 3.1, and You must inform recipients of
    the Executable Form how they can obtain a copy of such Source Code
    Form by reasonable means in a timely manner, at a charge no more
    than the cost of distribution to the recipient; and

(b) You may distribute such Executable Form under the terms of this
    License, or sublicense it under different terms, provided that the
    license for the Executable Form does not attempt to limit or alter
    the recipients' rights in the Source Code Form under this License.

3.3. Distribution of a Larger Work

You may create and distribute a Larger Work under terms of Your choice,
provided that You also comply with the requirements of this License for
the Covered Software. If the Larger Work is a combination of Covered
Software with a work governed by one or more Secondary Licenses, and the
Covered Software is not Incompatible With Secondary Licenses, this
License permits You to additionally distribute such Covered Software
under the terms of such Secondary License(s), so that the recipient of
the Larger Work may, at their option, further distribute the Covered
Software under the terms of either this License or such Secondary
License(s).

3.4. Notices

You may not remove or alter the substance of any license notices
(including copyright notices, patent notices, disclaimers of warranty,
or limitations of liability) contained within the Source Code Form of
the Covered Software, except that You may alter any license notices to
the extent required to remedy known factual inaccuracies.

3.5. Application of Additional Terms

You may choose to offer, and to charge a fee for, warranty, support,
indemnity or liability obligations to one or more recipients of Covered
Software. However, You may do so only on Your own behalf, and not on
behalf of any Contributor. You must make it absolutely clear that any
such warranty, support, indemnity, or liability obligation is offered by
You alone, and You hereby agree to indemnify every Contributor for any
liability incurred by such Contributor as a result of warranty, support,
indemnity or liability terms You offer. You may include additional
disclaimers of warranty and limitations of liability specific to any
jurisdiction.

4. Inability to Comply Due to Statute or Regulation
---------------------------------------------------

If it is impossible for You to comply with any of the terms of this
License with respect to some or all of the Covered Software due to
statute, judicial order, or regulation then You must: (a) comply with
the terms of this License to the maximum extent possible; and (b)
describe the limitations and the code they affect. Such description must
be placed in a text file included with all distributions of the Covered
Software under this License. Except to the extent prohibited by statute
or regulation, such description must be sufficiently detailed for a
recipient of ordinary skill to be able to understand it.

5. Termination
--------------

5.1. The rights granted under this License will terminate automatically
if You fail to comply with any of its terms. However, if You become
compliant, then the rights granted under this License from a particular
Contributor are reinstated (a) provisionally, unless and until such
Contributor explicitly and finally terminates Your grants, and (b) on an
ongoing basis, if such Contributor fails to notify You of the
non-compliance by some reasonable means prior to 60 days after You have
come back into compliance. Moreover, Your grants from a particular
Contributor are reinstated on an ongoing basis if such Contributor
notifies You of the non-compliance by some reasonable means, this is the
first time You have received notice of non-compliance with this License
from such Contributor, and You become compliant prior to 30 days after
Your receipt of the notice.

5.2. If You initiate litigation against any entity by asserting a patent
infringement claim (excluding declaratory judgment actions,
counter-claims, and cross-claims) alleging that a Contributor Version
directly or indirectly infringes any patent, then the rights granted to
You by any and all Contributors for the Covered Software under Section
2.1 of this License shall terminate.

5.3. In the event of termination under Sections 5.1 or 5.2 above, all
end user license agreements (excluding distributors and resellers) which
have been validly granted by You or Your distributors under this License
prior to termination shall survive termination.

************************************************************************
*                                                                      *
*  6. Disclaimer of Warranty                                           *
*  -------------------------                                           *
*                                                                      *
*  Covered Software is provided under this License on an "as is"       *
*  basis, without warranty of any kind, either expressed, implied, or  *
*  statutory, including, without limitation, warranties that the       *
*  Covered Software is free of defects, merchantable, fit for a        *
*  particular purpose or non-infringing. The entire risk as to the     *
*  quality and performance of the Covered Software is with You.        *
*  Should any Covered Software prove defective in any respect, You     *
*  (not any Contributor) assume the cost of any necessary servicing,   *
*  repair, or correction. This disclaimer of warranty constitutes an   *
*  essential part of this License. No use of any Covered Software is   *
*  authorized under this License except under this disclaimer.         *
*                                                                      *
************************************************************************

************************************************************************
*                                                                      *
*  7. Limitation of Liability                                          *
*  --------------------------                                          *
*                                                                      *
*  Under no circumstances and under no legal theory, whether tort      *
*  (including negligence), contract, or otherwise, shall any           *
*  Contributor, or anyone who distributes Covered Software as          *
*  permitted above, be liable to You for any direct, indirect,         *
*  special, incidental, or consequential damages of any character      *
*  including, without limitation, damages for lost profits, loss of    *
*  goodwill, work stoppage, computer failure or malfunction, or any    *
*  and all other commercial damages or losses, even if such party      *
*  shall have been informed of the possibility of such damages. This   *
*  limitation of liability shall not apply to liability for death or   *
*  personal injury resulting from such party's negligence to the       *
*  extent applicable law prohibits such limitation. Some               *
*  jurisdictions do not allow the exclusion or limitation of           *
*  incidental or consequential damages, so this exclusion and          *
*  limitation may not apply to You.                                    *
*                                                                      *
************************************************************************

8. Litigation
-------------

Any litigation relating to this License may be brought only in the
courts of a jurisdiction where the defendant maintains its principal
place of business and such litigation shall be governed by laws of that
jurisdiction, without reference to its conflict-of-law provisions.
Nothing in this Section shall prevent a party's ability to bring
cross-claims or counter-claims.

9. Miscellaneous
----------------

This License represents the complete agreement concerning the subject
matter hereof. If any provision of this License is held to be
unenforceable, such provision shall be reformed only to the extent
necessary to make it enforceable. Any law or regulation which provides
that the language of a contract shall be construed against the drafter
shall not be used to construe this License against a Contributor.

10. Versions of the License
---------------------------

10.1. New Versions

Mozilla Foundation is the license steward. Except as provided in Section
10.3, no one other than the license steward has the right to modify or
publish new versions of this License. Each version will be given a
distinguishing version number.

10.2. Effect of New Versions

You may distribute the Covered Software under the terms of the version
of the License under which You originally received the Covered Software,
or under the terms of any subsequent version published by the license
steward.

10.3. Modified Versions

If you create software not governed by this License, and you want to
create a new license for such software, you may create and use a
modified version of this License if you rename the license and remove
any references to the name of the license steward (except to note that
such modified license differs from this License).

10.4. Distributing Source Code Form that is Incompatible With Secondary
Licenses

If You choose to distribute Source Code Form that is Incompatible With
Secondary Licenses under the terms of this version of the License, the
notice described in Exhibit B of this License must be attached.

Exhibit A - Source Code Form License Notice
-------------------------------------------

  This Source Code Form is subject to the terms of the Mozilla Public
  License, v. 2.0. If a copy of the MPL was not distributed with this
  file, You can obtain one at http://mozilla.org/MPL/2.0/.

If it is not possible or desirable to put the notice in a particular
file, then You may include the notice in a location (such as a LICENSE
file in a relevant directory) where a recipient would be likely to look
for such a notice.

You may add additional accurate notices of copyright ownership.

Exhibit B - "Incompatible With Secondary Licenses" Notice
---------------------------------------------------------

  This Source Code Form is "Incompatible With Secondary Licenses", as
  defined by the Mozilla Public License, v. 2.0.
